| kspaceFirstOrder3D-OMP 1.1 The C++ implementation of the k-wave toolbox for the time-domain simulation of acoustic wave fields in 3D

- Main Page
- Related Pages
- Classes
- Files

- File List
- File Members

All Classes Files Functions Variables Typedefs Enumerations Friends Pages
Classes | Enumerations
MatrixContainer.h File Reference

The header file containing the matrix container. More...

`#include <string.h>`
`#include <map>`
`#include <MatrixClasses/BaseMatrix.h>`
`#include <MatrixClasses/BaseFloatMatrix.h>`
`#include <MatrixClasses/RealMatrix.h>`
`#include <MatrixClasses/ComplexMatrix.h>`
`#include <MatrixClasses/FFTWComplexMatrix.h>`
`#include <MatrixClasses/UXYZ_SGXYZMatrix.h>`
`#include <MatrixClasses/IndexMatrix.h>`
`#include <MatrixClasses/OutputHDF5Stream.h>`
`#include <Utils/MatrixNames.h>`
`#include <Utils/DimensionSizes.h>`
Include dependency graph for MatrixContainer.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
struct | TMatrixRecord
| A structure storing details about the matrix. The matrix container stores this structures. More...
class | TMatrixContainer
| Class implementing the matrix container. More...
class | TOutputStreamContainer
| A container for output streams. More...

## Enumerations
enum | TMatrixID { kappa, c2, p, ux_sgx, uy_sgy, uz_sgz, ux_shifted, uy_shifted, uz_shifted, duxdx, duydy, duzdz, dxudxn, dyudyn, dzudzn, dxudxn_sgx, dyudyn_sgy, dzudzn_sgz, rhox, rhoy, rhoz, rho0, dt_rho0_sgx, dt_rho0_sgy, dt_rho0_sgz, p0_source_input, sensor_mask_index, sensor_mask_corners, ddx_k_shift_pos, ddy_k_shift_pos, ddz_k_shift_pos, ddx_k_shift_neg, ddy_k_shift_neg, ddz_k_shift_neg, x_shift_neg_r, y_shift_neg_r, z_shift_neg_r, pml_x_sgx, pml_y_sgy, pml_z_sgz, pml_x, pml_y, pml_z, absorb_tau, absorb_eta, absorb_nabla1, absorb_nabla2, BonA, ux_source_input, uy_source_input, uz_source_input, p_source_input, u_source_index, p_source_index, transducer_source_input, delay_mask, p_sensor_raw, p_sensor_rms, p_sensor_max, p_sensor_min, p_sensor_max_all, p_sensor_min_all, ux_sensor_raw, uy_sensor_raw, uz_sensor_raw, ux_shifted_sensor_raw, uy_shifted_sensor_raw, uz_shifted_sensor_raw, ux_sensor_rms, uy_sensor_rms, uz_sensor_rms, ux_sensor_max, uy_sensor_max, uz_sensor_max, ux_sensor_min, uy_sensor_min, uz_sensor_min, ux_sensor_max_all, uy_sensor_max_all, uz_sensor_max_all, ux_sensor_min_all, uy_sensor_min_all, uz_sensor_min_all, Temp_1_RS3D, Temp_2_RS3D, Temp_3_RS3D, FFT_X_temp, FFT_Y_temp, FFT_Z_temp, FFT_shift_temp }
| Matrix identifers of all matrices in the k-space code.

## Detailed Description

Author
  Jiri Jaros
  Faculty of Information Technology
  Brno University of Technology
  jaros.nosp@m.jir@.nosp@m.fit.v.nosp@m.utbr.nosp@m..cz

Version
  kspaceFirstOrder3D 2.15

Date
  14 September 2012, 14:33 (created)
  26 September 2014, 17:10 (revised)

# License

This file is part of the C++ extension of the k-Wave Toolbox (http://www.k-wave.org).
Copyright (C) 2014 Jiri Jaros and Bradley Treeby

This file is part of k-Wave. k-Wave is free software: you can redistribute it and/or modify it under the terms of the GNU Lesser General Public License as published by the Free Software Foundation, either version 3 of the License, or (at your option) any later version.

k-Wave is distributed in the hope that it will be useful, but WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the GNU Lesser General Public License for more details.

You should have received a copy of the GNU Lesser General Public License along with k-Wave. If not, see http://www.gnu.org/licenses/.

Definition in file MatrixContainer.h.