<map id="GetSolverGridSize1D" name="GetSolverGridSize1D">
<area shape="rect" id="node2" href="$namespace_solver_c_u_d_a_kernels.html#a2ea9adf0fb0b3f6eb531b9ac28e211d4" title="Add transducer data source to X component. " alt="" coords="727,22,873,60"/>
<area shape="rect" id="node6" href="$namespace_solver_c_u_d_a_kernels.html#a3efe7d6d7931ba46617224fe1f088810" title="Add in velocity source terms. " alt="" coords="485,79,625,118"/>
<area shape="rect" id="node8" href="$namespace_solver_c_u_d_a_kernels.html#a60c1ef8bc0707b0c512a3f6680acd466" title="Add in pressure source term. " alt="" coords="485,142,625,180"/>
<area shape="rect" id="node10" href="$namespace_solver_c_u_d_a_kernels.html#aa23362d770671eba90da06aaeedcdaee" title="Compute velocity for the initial pressure problem. " alt="" coords="225,243,367,282"/>
<area shape="rect" id="node12" href="$namespace_solver_c_u_d_a_kernels.html#a0b757b9d45141d16ccbfdbf1cd62436a" title="Add initial pressure to p0 (as p0 source). " alt="" coords="196,180,396,219"/>
<area shape="rect" id="node13" href="$namespace_solver_c_u_d_a_kernels.html#a27b44d61b50bbddb337ba99ad5f8fe4a" title="Calculate three temporary sums in the new pressure formula, non&#45;linear absorbing case. " alt="" coords="193,368,399,407"/>
<area shape="rect" id="node16" href="$namespace_solver_c_u_d_a_kernels.html#ac488a028a20d1c5d80aa3924aed4ec93" title="Sum sub&#45;terms to calculate new pressure, non&#45;linear case. " alt="" coords="204,431,388,470"/>
<area shape="rect" id="node18" href="$namespace_solver_c_u_d_a_kernels.html#abc76a899893944dafac56d61931b99c0" title="Sum sub&#45;terms to calculate new pressure, linear case. " alt="" coords="213,494,379,532"/>
<area shape="rect" id="node21" href="$namespace_solver_c_u_d_a_kernels.html#aed2b5a8ac00b9f02d273d3d366df2329" title="Sum sub&#45;terms for new p, linear lossless case. " alt="" coords="197,306,395,344"/>
<area shape="rect" id="node23" href="$namespace_solver_c_u_d_a_kernels.html#a29220d466aeba455aab32b4d3839bd06" title="Calculate two temporary sums in the new pressure formula, linear absorbing case. " alt="" coords="204,619,388,658"/>
<area shape="rect" id="node25" href="$namespace_solver_c_u_d_a_kernels.html#a75b3ff4db44252d85be20eb0380232a1" title="Sum sub&#45;terms for new p, linear lossless case. " alt="" coords="207,556,385,595"/>
<area shape="rect" id="node3" href="$class_t_k_space_first_order3_d_solver.html#a2885754d4a24c82eaf9ca0e13f91c6aa" title="Compute the main time loop of the kspaceFirstOrder3D. " alt="" coords="939,176,1117,215"/>
<area shape="rect" id="node4" href="$class_t_k_space_first_order3_d_solver.html#a90ea773b837b769c59cf20b1be80465c" title="Compute the k&#45;space simulation. " alt="" coords="1166,176,1343,215"/>
<area shape="rect" id="node5" href="$main_8cpp.html#a3c04138a5bfe5d72780bb7e82a18e627" title="main" alt="" coords="1393,183,1442,208"/>
<area shape="rect" id="node7" href="$class_t_k_space_first_order3_d_solver.html#aeb07f402efe18850f1c1e8fcd25c7e7e" title="Add in velocity source. " alt="" coords="711,84,889,123"/>
<area shape="rect" id="node9" href="$class_t_k_space_first_order3_d_solver.html#aa834814be21fb24defcd8e6ed00be6c2" title="Add in pressure source. " alt="" coords="711,147,889,186"/>
<area shape="rect" id="node11" href="$class_t_k_space_first_order3_d_solver.html#aa5597bf6aeed1124ef9f16ae3971a69b" title="Calculate p0_ ource. " alt="" coords="466,204,643,243"/>
<area shape="rect" id="node14" href="$class_t_k_space_first_order3_d_solver.html#a6a004bf1bd70957cc619afb7f4deae7a" title="Calculate three temporary sums in the new pressure formula, non&#45;linear absorbing case. " alt="" coords="448,368,661,407"/>
<area shape="rect" id="node15" href="$class_t_k_space_first_order3_d_solver.html#ab2dc638bd9a19bd5e6d0ad1f6b77e26d" title="Compute acoustic pressure for nonlinear case. " alt="" coords="709,336,891,375"/>
<area shape="rect" id="node17" href="$class_t_k_space_first_order3_d_solver.html#a20bd4e6d3fddb078756e057d8643cfeb" title="Sum sub&#45;terms to calculate new pressure, non&#45;linear case. " alt="" coords="459,431,650,470"/>
<area shape="rect" id="node19" href="$class_t_k_space_first_order3_d_solver.html#ae4063b8e87bcba0a425fadf6009258c6" title="Sum sub&#45;terms to calculate new pressure, linear case. " alt="" coords="466,494,643,532"/>
<area shape="rect" id="node20" href="$class_t_k_space_first_order3_d_solver.html#a64c96500c6544db12dd6d43c43763f9e" title="Compute acoustic pressure for linear case. " alt="" coords="711,524,889,563"/>
<area shape="rect" id="node22" href="$class_t_k_space_first_order3_d_solver.html#ab783951bfe7bffdd76b3e014460cc4f0" title="Sum sub&#45;terms for new p, linear lossless case. " alt="" coords="453,306,657,344"/>
<area shape="rect" id="node24" href="$class_t_k_space_first_order3_d_solver.html#a82bc1b5e4b15241c59f2410d1bc29df0" title="Calculate two temporary sums in the new pressure formula, linear absorbing case. " alt="" coords="459,619,650,658"/>
<area shape="rect" id="node26" href="$class_t_k_space_first_order3_d_solver.html#ac6271c47cb8ff1f2a2646c3dc58065c0" title="Sum sub&#45;terms for new p, linear lossless case. " alt="" coords="462,556,647,595"/>
</map>
