k-Wave Toolbox |

## 3D Time Reversal Reconstruction For A Spherical Sensor Example

On this page…
Overview Simulating the data Running the reconstruction Interpolating incomplete sensor data

### Overview

This example demonstrates the use of k-Wave for the time-reversal reconstruction of a three-dimensional photoacoustic wave-field recorded over a spherical sensor. The sensor data is simulated and then time-reversed using `kspaceFirstOrder3D`. It builds on the 2D Time Reversal Reconstruction For A Circular Sensor and 3D Time Reversal Reconstruction For A Planar Sensor examples.

- open the file in the MATLAB Editor
- run the file in MATLAB

Back to Top

### Simulating the data

The sensor data is simulated using `kspaceFirstOrder3D` with an initial pressure distribution created using `makeBall`. A Cartesian sensor mask of 100 points evenly distributed around a sphere (using the Golden Section Spiral method) is created using `makeCartSphere`. A visualisation of the initial pressure and the sensor mask using `cart2grid` and `voxelPlot` is shown below.

Back to Top

### Running the reconstruction

A plot of the initial pressure distribution and the reconstructed distribution using time-reversal are shown below (the three displayed image planes intersect at the centre of ball shown above). The plot scale for the reconstructed image has the plot limits reduced by a factor of 20.

Back to Top

### Interpolating incomplete sensor data

The reconstruction can again be improved by interpolating the sensor data onto a continuous sensor surface. This is achieved using `interpCartData` and a binary sensor mask of a continuous sphere (created here using `makeSphere`) that is spatially equivalent to the Cartesian measurement grid. This function calculates the equivalent time-series at the sensor positions on the binary sensor mask from those on the Cartesian sensor mask via interpolation (nearest neighbour is used by default).

    % create a binary sensor mask of an equivalent continuous sphere
    pixel_radius = round(sensor_radius/kgrid_recon.dx);
    binary_sensor_mask = makeSphere(kgrid_recon.Nx, kgrid_recon.Ny, kgrid_recon.Nz, pixel_radius);

    % interpolate data to remove the gaps and assign to time reversal data
    sensor.time_reversal_boundary_data = interpCartData(kgrid_recon, sensor_data, sensor_mask, binary_sensor_mask);

Details of the interpolation are printed to the command line.

    Interpolating Cartesian sensor data...
      interpolation mode: nearest
      number of Cartesian sensor points: 100
      number of binary sensor points: 4234
      computation completed in 0.075839s

The reconstruction after interpolation is shown below. The plot limits are set to match those of the initial pressure plot shown above.

Back to Top

© 2009-2012 Bradley Treeby and Ben Cox.