k-Wave Toolbox |

## 3D Time Reversal Reconstruction For A Planar Sensor Example

On this page…
Overview Simulating the sensor data Performing the reconstruction

### Overview

This example demonstrates the use of k-Wave for the reconstruction of a three-dimensional photoacoustic wave-field recorded over a planar array of sensor elements. The sensor data is simulated and then time-reversed using `kspaceFirstOrder3D`. It builds on the 3D FFT Reconstruction For A Planar Sensor and 2D Time Reversal Reconstruction For A Line Sensor examples.

- open the file in the MATLAB Editor
- run the file in MATLAB

Back to Top

### Simulating the sensor data

The sensor data is simulated using `kspaceFirstOrder3D` in the same way as in preceding examples. The utilised initial pressure distribution and the sensor mask are shown in 3D FFT Reconstruction For A Planar Sensor. The time-reversal reconstruction is then performed by assigning the time varying pressure recorded over the detector array to `sensor.time_reversal_boundary_data`.

    % run the simulation
    sensor_data = kspaceFirstOrder3D(kgrid, medium, source, sensor, input_args{:});

    % reset the initial pressure
    source.p0 = 0;

    % assign the time reversal data
    sensor.time_reversal_boundary_data = sensor_data;

    % run the time-reversal reconstruction
    p0_recon = kspaceFirstOrder3D(kgrid, medium, source, sensor, input_args{:});

A plot of the reconstructed initial pressure distribution with a positivity condition is shown below.

Back to Top

© 2009-2014 Bradley Treeby and Ben Cox.