# envelopeDetection

Extract signal envelope using the Hilbert Transform.

## Syntax

    env = envelopeDetection(x)

## Description

`envelopeDetection` applies the Hilbert transform to extract the envelope from an input vector `x`. If `x` is a matrix, the envelope along each row is returned. For example, running the code

    % create tone burst
    x = toneBurst(10e6, 0.5e6, 10);

    % plot tone burst and envelope
    figure;
    plot(0:length(x) - 1, x, 'k-', 0:length(x) - 1, envelopeDetection(x), 'r-');
    legend('Input Signal', 'Envelope');

produces the output

## Inputs

`x` | input function

## Outputs

`env` | envelope of input function

## See Also

`fft`